I faced some problem when completing this exercise. Please keep in mind when you are trying to implement this code.

1. Use micropython 2023 version. The file is given (RPI\_PICO\_W-20231005-v1.21.0.uf2) in the folder.
2. The ‘simple.py’ and ‘robust.py’ file are umqtt files. Save this file inside pico w memory (not in your own pc) as ‘simple.py’ and ‘robust.py’ respectively. I save it as ‘umqtt.simple.py’ and then tried to import it, it did not worked.
3. Save ‘config.py’ file inside pico w memory.
4. You do not need to save ‘hivemq.py’ file anywhere. Just open it in ‘Thonny’ and run it. It should work fine.
5. Do not use 5G band wifi. Use 2.4G band for pico w. Pico w do not connect 5G network.
6. You can follow the execise-3 pdf. Everything should work.